For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear window wiper arm. Refer to Rear Window Wiper Arm Replacement .
3. Remove the hatchback door lower garnish molding.
4. Remove the bolts and the rear wiper motor.
5. Disconnect the electrical connector.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the electrical connector.
2. Install the rear wiper motor with the bolts.

Tighten
Tighten the wiper motor bolts to 9 N·m (80 lb in).

3. Install the hatchback door lower garnish molding.
4. Install the rear window wiper arm. Refer to Rear Window Wiper Arm Replacement .
5. Connect the negative battery cable.