For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Caliper Piston Minimum Diameter | 54 mm | 2.12 in
Disc Type | Ventilated
Discard Thickness for 236 mm (9.29 in) Diameter Rotor | 18 mm | 0.709 in
Discard Thickness for 256 mm (10.08 in) Diameter Rotor | 22 mm | 0.866 in
Maximum Assembled Lateral Runout - Installed | 0.06 mm | 0.002 in
Maximum Groove Depth | 0.40 mm | 0.016 in
Maximum Lateral Runout - Not Installed | 0.03 mm | 0.001 in
Maximum Thickness Variation | 0.10 mm | 0.004 in
New Rotor Thickness - 236 mm (9.29 in) Diameter Rotor | 20 mm | 0.787 in
New Rotor Thickness - 256 mm (10.08 in) Diameter Rotor | 24 mm | 0.945 in
Rotor Diameter - Larger Size with SACL500 Stamping | 256 mm | 10.08 in
Rotor Diameter - Smaller Size with SACL485F Stamping | 236 mm | 9.29 in