For 1990-2009 cars

## Clutch Rotor and Bearing Removal V5 Compressor

#### Tools Required

• | J 6083 Snap Ring Pliers

• | J 8092 Driver Handle

• | J 9398-A Bearing Remover

• | J 33020 Pulley Puller

### Disassembly Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
3. Remove the compressor. Refer to Air Conditioning Compressor Replacement .
4. Remove the clutch drive plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
5. Remove the pulley rotor and the bearing assembly retaining ring using the J 6083 .
6. Install the J 33020 (1) into the inner circle of slots in the pulley rotor. Turn the J 33020 (1) clockwise in the slots to engage the puller tangs with the segments between the slots in the rotor.
7. Hold the J 33020 (1) in place and tighten the puller bolt against the compressor shaft to remove the pulley rotor and the bearing assembly.

Notice: The rotor hub must be properly supported to prevent damage to the pulley rotor during bearing removal.

8. Remove the puller bolt from the J 33020 . With the puller tangs still engaged in the rotor slots, invert the assembly onto a solid flat surface or blocks.
9. Drive the bearing out of the rotor hub with the J 9398-A (2) and the J 8092 (1).

## Clutch Rotor and Bearing Removal SP10 Compressor

#### Tools Required

J 9553-01 O-Ring Remover

1. Remove the clutch and drive assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
2. Remove the shims using the J 9553-01 O-ring remover.
3. Remove the pulley ring retainer using the snap ring pliers (1).
4. Pull the pulley groove with both hands until the pulley and bearing assembly is free.