For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the chime module.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the chime module with the screws.

Tighten
Tighten the chime module screws to 3.5 N·m (31 lb in).

3. Connect the negative battery cable.