For 1990-2009 cars

### Removal Procedure

1. Disconnect the cruise control clutch pedal switch electrical connector.
2. Turn the switch 90 degrees counterclockwise and remove.

### Installation Procedure

1. Position the cruise control clutch switch in the pedal support, then turn the switch 90 degrees clockwise.
2. Connect the cruise control clutch pedal switch electrical connector.
3. Adjust the cruise control clutch pedal switch. Refer to Clutch Pedal Cruise Control Release Switch Adjustment .