For 1990-2009 cars

### Removal Procedure

1. Open and suitably support the hatchback door.
2. Disconnect the hatchback door grommet, the electrical connector, and the washer hose.
3. Remove the gas support assemblies from the hatchback door and the body. Refer to Liftgate Strut Replacement .
4. With the aid of another technician, remove the bolts and the hatchback door from the hinges.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. With the aid of another technician, install the hatchback door to the hinges with the bolts.

Tighten
Tighten the hatchback door hinge bolts to 20 N·m (15 lb ft).

2. Install the gas support assemblies to the hatchback door and the body. Refer to Liftgate Strut Replacement .
3. Connect the hatchback door electrical connector, the washer hose, and the grommet.
4. Close the hatchback door.