For 1990-2009 cars

### Removal Procedure

1. Remove the seat back. Refer to Front Seat Back Replacement .
2. Remove the seat cushion bolts.
3. Remove the cushion from the seat adjuster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat cushion to the seat adjuster with the bolts.

Tighten
Tighten the seat cushion bolts to 25 N·m (18 lb ft).

2. Install the seat back. Refer to Front Seat Back Replacement .