For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment.
2. Remove the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement .
3. Remove the bolts that secure the lock striker.
4. Pull the lock striker out.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock striker with the bolts.

Tighten
Tighten the luggage compartment lock striker bolts to 8 N·m (71 lb in).

2. Instal the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement .