For 1990-2009 cars

Check for a leak in the area of transaxle case and sealing and then check fluid level and condition after removing oil level plug.

1. Operate the engine until normal operating temperature.

Specifications
The coolant temperature is 80-90°C (176-194°F).

Danger: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

2. Stop the engine and raise the vehicle.
3. Remove the oil level plug (2) and check the fluid level.
4. The fluid should slightly flow out from the oil level plug hole.
5. If the level is low, add SAE 75W90 manual transmission fluid through the oil level plug hole until the fluid begins to run out.
6. If the fluid is contaminated or discolored, replace it with the recommended fluid.
7. Install the oil level plug and tighten to 28 N·m (21 lb ft).