For 1990-2009 cars

Application | Description
--- | ---
Starter

- No Load Test @ 12 volts (1.4L/1.5L SOHC and 1.4L/1.6L DOHC)

Maximum 90 amps

- Drive Pinion Speed (1.4L/1.5L SOHC and 1.4L/1.6L DOHC)

Minimum 2,600 RPM

- No Load Test 9 volts (1.2L)

Maximum 150 amps

- Drive Pinion Speed (1.2L)

Minimum 2,000 RPM

Solenoid

- Hold-in Windings @ 12 volts

12-20 amps

- Pull-in Windings @ 12 volts

60-90 amps