For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
3. Disconnect the electrical connector.
4. Remove the actuating rod by snapping it out of the lever with needle-nose pliers.
5. Remove the air temperature actuator retaining screws.
6. Remove the air temperature actuator.

### Installation Procedure

1. Install the air temperature actuator.
2. Install the retaining screws and tighten.
3. Install the actuating rod.
4. Connect the electrical connector.
5. Install the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
6. Connect the negative battery cable.