For 1990-2009 cars

### Removal Procedure

1. Remove the center console. Refer to Front Floor Console Replacement.
2. Remove the heating and air conditioning controls. Refer to Heater and Air Conditioning Control Replacement.
3. Remove the four screws and the cupholder assembly (1) from the instrument panel.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the cupholder assembly (1) with the four screws and tighten to 2.5 N·m (22 lb in).
2. Install the heating and air conditioning controls. Refer to Heater and Air Conditioning Control Replacement.
3. Install the center console. Refer to Front Floor Console Replacement.