For 1990-2009 cars

## Rear Door Lock Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Disconnect the inside door handle and the lock rods.
4. Disconnect the outside door handle and the lock rods.
5. Remove the bolts and the guide rail.
6. Remove the screws and the lock.
7. Disconnect the electrical connector.
8. Disconnect the lock rods at the lock.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear door lock with the screws and tighten to 8 N·m (71 lb in).
2. Connect the electrical connector.
3. Install the guide rail with the bolts and tighten to 7 N·m (62 lb in).
4. Connect the outside door handle and the lock rods.
5. Connect the inside door handle and the lock rods.
6. Install the water deflector. Refer to Door Water Deflector Replacement.
7. Connect the negative battery cable.

## Rear Door Lock Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door water deflector. Refer to Door Water Deflector Replacement.
3. Disconnect the inside door handle and the lock rods.
4. Disconnect the outside door handle and the lock rods.
5. Remove the bolts and the guide rail.
6. Remove the screws and the lock.
7. Disconnect the electrical connector.
8. Disconnect the lock rods at the lock.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear door lock with the screws and tighten to 8 N·m (71 lb in).
2. Connect the electrical connector.
3. Install the guide rail with the bolts and tighten to 7 N·m (62 lb in).
4. Connect the outside door handle and the lock rods.
5. Connect the inside door handle and the lock rods.
6. Install the door water deflector. Refer to Door Water Deflector Replacement.
7. Connect the negative battery cable.