For 1990-2009 cars

## Rear Compartment Lid Lock Cylinder Replacement Hatchback

### Removal Procedure

1. Remove the hatchback door lower garnish molding, if equipped.
2. Disconnect the lock rod.
3. Remove the nuts and the lock cylinder.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock cylinder with the nuts.

Tighten
Tighten the luggage compartment lock cylinder nuts to 3 N·m (27 lb in).

2. Connect the lock rod.
3. Install the hatchback door lower garnish molding, if equipped.

## Rear Compartment Lid Lock Cylinder Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the clips and the rear compartment lid trim.
3. Disconnect the electrical connector.
4. Disconnect the lock rod.
5. Remove the bolt and the lock cylinder.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock cylinder with the bolt.

Tighten
Tighten the luggage compartment lock cylinder bolt to 4 N·m (35 lb in).

2. Connect the lock rod.
3. Install the rear compartment lid trim with the clips.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .