For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the exhaust gas recirculation (EGR) valve electrical connector.
3. Remove the bolts and the EGR valve.

### Installation Procedure

1. Clean the cylinder head mating surface.
2. Install a new EGR valve gasket.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the EGR valve with the retaining bolts.

Tighten
Tighten the EGR valve retaining bolts to 30 N·m (22 lb ft).

4. Connect the EGR valve electrical connector.
5. Connect the negative battery cable.