For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the floor console. Refer to Front Floor Console Replacement.
3. Remove the cable adjusting nut.
4. Disconnect the shift control cable from the shift control lever assembly.
5. Remove the shift control cable retaining E-ring.
6. Disconnect the shift control cable from the park/neutral position (PNP) switch.
7. Remove the E-ring from the shift control cable bracket and disconnect the shift control cable.
8. Disconnect the shift control cable from the shift control cable fastener.
9. Remove the shift control cable from the vehicle.

### Installation Procedure

1. Install the shift control cable to the vehicle.
2. Connect the shift control cable to the shift control cable fastener.
3. Install the E-ring to the shift control cable bracket and connect the shift control cable.
4. Connect the shift control cable to the PNP switch.
5. Install the shift control cable retaining E-ring.
6. Connect the shift control cable to the shift control lever assembly.

Notice: Refer to Fastener Notice in the Preface section.

7. Install the cable adjusting nut.

Tighten
Tighten the cable adjusting nut to 8 N·m (71 lb in).

8. Install the trim panel to the floor console. Refer to Front Floor Console Replacement.
9. Connect the negative battery cable.