For 1990-2009 cars

## High Beams Inoperative Hatchback

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Test the high beam headlamps in the flash-to-pass mode. Do the high beam headlamps work in the flash-to-pass mode? | -- | Go to Step 2 | Go to Step 3
2 | Replace the headlamp combination switch. Is the repair complete? | -- | System OK | --
3 | Test fuses EF25 and EF26. Is fuse EF25 and EF26 open? | -- | Go to Step 4 | Go to Step 5
4 |

1. Test for a short circuit. Repair the short circuit, if necessary.
2. Replace the fuse.

Is the repair complete?

--

System OK

--

5 |

1. Turn ON the high beam headlamps.
2. Measure the voltage at fuse EF25 and EF26.

Does the voltage available at fuse EF25 and EF26 equal the value specified?

11-14 V

Go to Step 7

Go to Step 6

6 | Temporarily substitute the illumination lamp relay in place of the headlamp high relay. Do the headlamps operate with the substituted relay? | -- | Go to Step 7 | Go to Step 8
7 | Reinstall the illumination lamp relay in its original position, and install a new headlamp relay. Is the repair complete? | -- | System OK | --
8 |

1. Install the headlamp high relay.
2. Measure the voltage at headlamp switch connector terminal 4.

Does the voltage equal the value specified?

11-14 V

Go to Step 10

Go to Step 9

9 | Repair the open circuit between headlamp high relay terminal 86 and headlamp switch connector terminal 4. Is the repair complete? | -- | System OK | --
10 |

1. Disconnect the headlamp connector.
2. Turn the headlamp switch to the high-beam position.
3. Use an ohmmeter to measure the continuity between terminals 6 and 4 of the headlamp switch.

Does the ohmmeter indicate continuity?

--

Go to Step 11

Go to Step 2

11 |

1. Connect the headlamp switch connector.
2. Turn the headlamp switch to the high-beam position.
3. Measure the voltage at the light switch connector terminal 2.

Does the voltage equal the value specified?

11-14 V

Go to Step 13

Go to Step 12

12 | Repair the open circuit between the headlamp switch connector terminal 6 and light switch connector terminal 2. Is the repair complete? | -- | System OK | --
13 |

1. Disconnect the light switch connector.
2. Turn the headlamp switch to the high-beam position.
3. Use an ohmmeter to measure the continuity between terminals 2 and 3 of the light switch.

Does the ohmmeter indicate continuity?

--

Go to Step 14

Go to Step 2

14 | Repair the open circuit between ground and the light switch connector terminal 3. Is the repair complete? | -- | System OK | --
15 |

1. Turn ON the high beam headlamps.
2. Measure the voltage at headlamp terminal 1 with the high beams selected.

Does the voltage available at the headlamp connector terminal 1 equal the value specified?

11-14 V

Go to Step 17

Go to Step 16

16 | Repair the open circuit between fuse EF19 and the high beam headlamps. Is the repair complete? | -- | System OK | --
17 |

1. Disconnect the headlamp connectors.
2. Connect an ohmmeter between the ground and the headlamp connector terminal 3.

Does the ohmmeter indicate continuity?

--

Go to Step 19

Go to Step 18

18 | Repair the open circuit between the ground and the headlamp connector terminal 3. Is the repair complete? | -- | System OK | --
19 | Replace the faulty headlamps. Refer to Headlamp Replacement . Is the repair complete? | -- | System OK | --

## High Beams Inoperative Notchback

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Check the high beam headlamps in the flash-to-pass mode. Do the high beam headlamps work in the flash-to-pass mode? | -- | Go to Step 2 | Go to Step 3
2 | Replace the headlamp combination switch. Is the repair complete? | -- | System OK | --
3 | Temporarily substitute the illumination lamp relay in place of the headlamp high relay. Do the headlamps operate with the substitute relay? | -- | Go to Step 4 | Go to Step 5
4 | Reinstall the illumination lamp relay in its original position and install a new headlamp relay. Is the repair complete? | -- | System OK | --
5 |

1. Install the headlamp high relay.
2. Check the voltage at headlamp switch connector terminal 4.

Does the voltage equal the value specified?

11-14V

Go to Step 7

Go to Step 6

6 | Repair the open circuit between headlamp high relay terminal 86 and headlamp switch connector terminal 4. Is the repair complete? | -- | System OK | --
7 |

1. Disconnect the headlamp switch connector.
2. Turn the headlamp switch to the high-beam position.
3. Use an ohmmeter to check the continuity between terminals 6 and 4 of the headlamp switch.

Is the resistance within the specified value?

<1.0 ohms

Go to Step 8

Go to Step 2

8 |

1. Connect the headlamp switch connector.
2. Turn the headlamp switch to the high-beam position.
3. Check the voltage at the light switch connector terminal 2.

Does the voltage equal the value specified?

11-14V

Go to Step 10

Go to Step 9

9 | Repair the open circuit between the headlamp switch connector terminal 6 and light switch connector terminal 2. Is the repair complete? | -- | System OK | --
10 |

1. Disconnect the light switch connector.
2. Turn the headlamp switch to the high-beam position.
3. Use an ohmmeter to check the continuity between terminals 2 and 3 of the light switch.

Is the resistance within the specified value?

<1.0 ohms

Go to Step 11

Go to Step 2

11 | Repair the open circuit between ground and the light switch connector terminal 3. Is the repair complete? | -- | System OK | --
12 |

1. Turn the high beam headlamps on.
2. Check the voltage at headlamp terminal 1 with the high beams selected.

Doe the voltage available at the headlamp connector terminal 1 equal the value specified?

11-14V

Go to Step 14

Go to Step 13

13 | Repair the open circuit between fuse Ef23 and the high beam headlamps. Is the repair complete? | -- | System OK | --
14 |

1. Disconnect the headlamp connectors.
2. Connect an ohmmeter between the ground and the headlamp connector terminal 3.

Is the resistance within the specified value?

<1.0 ohms

Go to Step 16

Go to Step 15

15 | Repair the open circuit between the ground and the headlamp connector terminal 3. Is the repair complete? | -- | System OK | --
16 | Replace the faulty headlamps. Is the repair complete? | -- | System OK | --