For 1990-2009 cars

## DTC P0727 European or North American Emissions

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0727 Engine Speed Signal

### Conditions for Setting the DTC

• | The transmission control module (TCM) detects that malfunction of engine speed signal for 2 seconds.

• | No DTC U2105

### Action Taken When the DTC Sets

• | The TCM will request the illumination of the malfunction indicator lamp (MIL) and store the DTC when the TCM detects a failure on the first ignition cycle.

• | No engine torque reduction control

• | No lock-up

• | No engagement pressure control

• | No 4th gear

• | No self-learning control

• | No timing solenoid control for N-D

• | The TCM judges the engine revolution is 0 RPM.

### Conditions for Clearing the DTC

• | The TCM turns OFF the MIL when no further failures are detected on the next ignition cycle.

• | The scan tool can clear the DTC from the TCM history.

• | The TCM clears the DTC from the TCM history memory after 40 consecutive ignition cycles without fault.

### Cause of Failure

• | The wiring harness or connector between the engine control module (ECM) and the TCM

• | The ECM

• | The TCM

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Automatic Transmission? | -- | Go to Step 2 | Go to Diagnostic System Check - Automatic Transmission
2 |

1. Turn OFF the ignition.
2. Install the scan tool.
3. With the engine OFF, turn the ignition switch to the ON position.
4. Select Store Freeze Frame/Failure Records from the DTC Information menu.
5. Store Freeze Frame/Failure Records.
6. Select Clear DTC Information from the DTC Information menu.
7. Clear the DTC information.
8. Perform one vehicle drive cycle.

Is the malfunction indicator lamp (MIL) ON?

--

Go to Step 3

Go to Step 7

3 |

1. Select Request DTC by Status from the DTC Information menu.
2. Request DTC by Status.

Is DTC P0727 displayed?

--

Go to Step 4

Go to Step 7

4 |

1. Turn OFF the ignition.
2. Disconnect the transmission control module (TCM) wiring connector and the engine control module (ECM) wiring connector.
3. Measure the resistance between terminal A17 of the TCM wiring connector and terminal K14, B14, or 88 of the ECM wiring connector.
4. Measure the resistance between terminal A7 of the TCM wiring connector and terminal K15, B30, or 57 of the ECM wiring connector.

Is the resistance within the specified value?

0 Ω

Go to Step 5

Go to Step 6

5 |

1. Turn ON the ignition.
2. Measure the voltage of terminal A17.
3. Measure the voltage of terminal A7.

Is the voltage within the specified range?

11-14 V

Go to Step 6

Go to Step 8

6 | Repair the malfunctioning terminals, as necessary. Did you complete the repair? | -- | System OK | --
7 | Repair the temporary connection failure of the connector. Refer to Transmission Control Module Replacement. Did you complete the repair? | -- | System OK | --
8 | Inspect the engine for proper operation. Was a condition found? | -- | Go to Diagnostic System Check - Vehicle | Go to Step 9
9 |

1. Replace the TCM. Refer to Transmission Control Module Replacement.
2. Turn OFF the ignition.
3. Turn ON the ignition.
4. Inspect if DTC P0727 is set.

Is the DTC set?

--

Go to Step 10

Go to Step 11

10 | Replace the ECM. Refer to Control Module References. Did you complete the replacement? | -- | Go to Step 11 | --
11 |

1. After the repair, use a scan tool Clear Info function and road test the vehicle.
2. Review the DTC info.

Has the last test failed or is the current DTC displayed?

--

Go to Step 2

System OK

## DTC P0727 Non European or N. American Emissions

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0727 Engine Speed Signal

### Conditions for Setting the DTC

• | The transmission control module (TCM) detects that malfunction of the engine speed signal for 2 seconds.

• | No DTC U2105

### Action Taken When the DTC Sets

• | The TCM will request the illumination of the hold lamp and store the DTC when the TCM detects a failure on the 1st ignition cycle.

• | No engine torque reduction control

• | No lock-up

• | No engagement pressure control

• | No 4th gear

• | No self-learning control

• | No timing solenoid control for N-D

• | The TCM judges the engine revolution is 0 RPM.

### Conditions for Clearing the DTC

• | The TCM turns OFF the hold lamp when no further failures are detected on the next ignition cycle.

• | The scan tool can clear the DTC from the TCM history.

• | The TCM clears the DTC from the TCM history memory after 40 consecutive ignition cycles without fault.

### Cause of Failure

• | The wiring harness or connector between the engine control module (ECM) and the TCM

• | The ECM

• | The TCM

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Automatic Transmission? | -- | Go to Step 2 | Go to Diagnostic System Check - Automatic Transmission
2 |

1. Turn OFF the ignition.
2. Install the scan tool.
3. With the engine OFF, turn the ignition switch to the ON position.
4. Select Store Freeze Frame/Failure Records from the DTC Information menu.
5. Store Freeze Frame/Failure Records.
6. Select Clear DTC Information from the DTC Information menu.
7. Clear the DTC information.
8. Perform one vehicle drive cycle.

Is the hold lamp ON?

--

Go to Step 3

Go to Step 7

3 |

1. Select Request DTC by Status from the DTC Information menu.
2. Request DTC by Status.

Is DTC P0727 displayed?

--

Go to Step 4

Go to Step 7

4 |

1. Turn OFF the ignition.
2. Disconnect the transmission control module (TCM) wiring connector and the engine control module (ECM) wiring connector.
3. Measure the resistance between terminal A17 of the TCM wiring connector and terminal K14, B14, or 88 of the ECM wiring connector.
4. Measure the resistance between terminal A7 of the TCM wiring connector and terminal K15, B30, or 57 of the ECM wiring connector.

Is the resistance within the specified value?

0 Ω

Go to Step 5

Go to Step 6

5 |

1. Turn ON the ignition.
2. Measure the voltage of terminal A17.
3. Measure the voltage of terminal A7.

Is the voltage within the specified range?

11-14 V

Go to Step 6

Go to Step 8

6 | Repair the malfunctioning terminals, as necessary. Did you complete the repair? | -- | System OK | --
7 | Repair the temporary connection failure of the connector. Refer to Transmission Control Module Replacement. Did you complete the repair? | -- | System OK | --
8 | Inspect the engine for proper operation. Was a condition found? | -- | Go to Diagnostic System Check - Vehicle | Go to Step 9
9 |

1. Replace the TCM. Refer to Transmission Control Module Replacement.
2. Turn OFF the ignition.
3. Turn ON the ignition.
4. Inspect if DTC P0727 is set.

Is the DTC set?

--

Go to Step 10

Go to Step 11

10 | Replace the ECM. Refer to Control Module References. Did you complete the replacement? | -- | Go to Step 11 | --
11 |

1. After the repair, use a scan tool Clear Info Function and road test the vehicle.
2. Review the DTC info.

Has the last test failed or is the current DTC displayed?

--

Go to Step 2

System OK