For 1990-2009 cars

#### Special Tools

J 28467-B (DW-117) Universal Engine Support Fixture

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the upper radiator cover.
3. Remove the right front splash shield.
4. Support the engine assembly using the J 28467-B (1).
5. Remove the engine mount bracket retaining bolts.
6. Remove the engine mount retaining nuts.
7. Lower the engine.
8. Remove the engine mount.

### Installation Procedure

1. Install the engine mount.
2. Raise the engine.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the engine mount retaining nuts.

Tighten
Tighten the engine mount retaining nuts to 40 N·m (30 lb ft).

4. Install the engine mount bracket retaining bolts.

Tighten
Tighten the engine mount bracket retaining bolts to 55 N·m (41 lb ft).

5. Remove J 28467-B (1).
6. Install the right front splash shield.
7. Install the upper radiator cover.
8. Connect the negative battery cable.