For 1990-2009 cars

### Circuit Description

When the ignition switch is turned to ON, the sensing and diagnostic module (SDM) will perform a turn-on test to diagnose critical malfunctions within the SDM itself.

These test ignition and deployment loop voltages are measured to ensure that they are within their normal voltage ranges. The SDM monitors the voltages at the driver low and the passenger low to detect shorts to ground or voltage in the deploy loops.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC B1102 Battery Voltage Low

### Conditions for Running the DTC

Ignition voltage is within the normal operating voltage range.

### Conditions for Setting the DTC

The voltage supplied from the battery is lower than 10.6 volts.

### Action Taken When the DTC Sets

The SDM commands the AIR BAG indicator ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section. Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section. Schematic Reference: SIR Schematics Connector End View Reference: SIR Connector End Views
1 | Did you perform a Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Inspect fuse F1. Is the fuse blown? | -- | Go to Step 3 | Go to Step 4
3 | Replace fuse F1. Is the replacement complete? | -- | Go to Step 11 | --
4 |

1. Confirm the ignition switch is ON.
2. Measure the voltage from fuse F1.

Is the voltage less than the specified value?

10.6 V

Go to Step 5

Go to Step 6

5 | Repair the power supply and the wiring to fuse F1. Is the repair complete? | -- | Go to Step 11 | --
6 |

1. Confirm the ignition switch is OFF.
2. Disconnect the connector of the steering wheel module coil.
3. Disconnect the connector of the I/P module.
4. Disconnect the connector of the sensing and diagnostic module (SDM).
5. Confirm the ignition switch is ON.
6. Measure the voltage between terminal 26 of the SDM connector and the ground.

Is the voltage less than the specified value?

10.6 V

Go to Step 7

Go to Step 9

7 |

1. Disconnect the C216.
2. Confirm the ignition switch is ON.
3. Measure the voltage from terminal 7 of C216.

Is the voltage less than the specified value?

10.6 V

Go to Step 8

Go to Step 10

8 | Repair the wire between the fuse F1 and the terminal 7 of connector C216. Is the repair complete? | -- | Go to Step 11 | --
9 | Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement . Is the replacement complete? | -- | Go to Step 11 | --
10 | Repair the wire between the SDM terminal 26 and the terminal 7 of connector C214. Is the replacement complete? | -- | Go to Step 11 | --
11 |

1. Reconnect all SIR components.
2. Verify that all components, connectors and connector position assurances (CPAs) are properly mounted.
3. Use the scan tool in order to clear the DTCs.
4. Operate the vehicle within the Conditions for Running the DTC, as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK