For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accessory Mounting Bracket Bolts | 37 N·m | 27 lb ft
Camshaft Position Sensor Bolt | 12 N·m | 106 lb in
Crankshaft Position (CKP) Sensor Bolt | 6.5 N·m | 58 lb in
Engine Control Module (ECM) Nuts | 7 N·m | 62 lb in
Engine Coolant Temperature Sensor | 17.5 N·m | 13 lb ft
Evaporative Emission Canister Bracket Retaining Bolt | 8 N·m | 71 lb in
Evaporative Emission Canister Flange Bolt | 20 N·m | 16 lb ft
Evaporative Emission Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Evaporative Emission Vent Solenoid Bolt | 8.5 N·m | 75 lb in
Exhaust Gas Recirculation Retaining Bolts | 30 N·m | 22 lb ft
Exhaust Gas Recirculation Retaining Bolts | 22 N·m | 16 lb ft
Exhaust Gas Recirculation Retaining Nuts | 10 N·m | 89 lb in
Fuel Filter Bracket Bolt | 4 N·m | 35 lb in
Fuel Pressure Regulator Retaining Screw | 12 N·m | 106 lb in
Fuel Pump Retaining Bolts | 4 N·m | 35 lb in
Fuel Tank Retaining Bolts | 20 N·m | 15 lb ft
Fuel Rail Bolt | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Idle Air Control Valve Retaining Bolts | 3 N·m | 27 lb in
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) Bolt | 20 N·m | 15 lb ft
Map Sensor Retaining Bolts | 10 N·m | 89 lb in
Oil Pressure Switch Fitting | 30 N·m | 22 lb ft
Spark Plug Cover Bolts | 3 N·m | 27 lb in
Throttle Body Nuts | 10.5 N·m | 93 lb in
Throttle Position Sensor Retaining Bolts | 3 N·m | 24 lb in