For 1990-2009 cars

### Removal Procedure

1. Remove the exhaust gas recirculation (EGR) pipe mounting bolts from the intake manifold.
2. Remove the EGR pipe mounting bolts from the EGR valve.
3. Raise and suitable support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the lower mounting bolt attaching the EGR pipe to the intake manifold.
5. Remove the EGR pipe.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the EGR pipe and the lower bolt attaching the EGR pipe to the intake manifold.

Tighten
Tighten the EGR pipe mounting bolt to 12 N·m (106 lb in).

2. Install the EGR pipe mounting bolts to the EGR valve.

Tighten
Tighten the EGR pipe to EGR valve mounting bolts to 10 N·m (89 lb in).

3. Lower the vehicle.
4. Install the EGR pipe mounting bolts to the intake manifold.

Tighten
Tighten the EGR pipe to intake manifold mounting bolts to 12 N·m (106 lb in).