For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headliner. Refer to Headlining Trim Panel Replacement.
3. Remove the drain hoses.
4. Remove the strap.
5. Disconnect the electrical connector.
6. Remove the bolts and the motor.
7. Disconnect the electrical connector.
8. Remove the strap.
9. Remove the motor control module.
10. Remove the bolts and the sunroof housing from the vehicle.
11. Remove the drain channel.
12. Remove the sunshade.

### Installation Procedure

1. Install the sunshade.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the sunroof housing and tighten to 7 N·m (62 lb in)..
3. Install the motor control module.
4. Manually position the sunroof glass in the fully closed position.

Note: The sunroof motor assembly must be in the fully closed position before installation.

5. Install the motor and tighten to 5 N·m (44 lb in).
6. Install the drain hoses.
7. Install the headliner. Refer to Headlining Trim Panel Replacement.
8. Connect the negative battery cable.