For 1990-2009 cars

#### Tools Required

KM-507-C Ball Joint Remover

### Removal Procedure

1. Remove the outer tie rod hex nut and disconnect the outer tie rod from the steering knuckle using the KM-507-C .

Important: Before loosening the tie rod lock nut, mark the position of the lock nut for easy alignment after the installation procedure.

2. Loosen the tie rod lock nuts and remove the outer tie rod.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outer tie rod with the lock nuts.

Tighten
Tighten the lock nuts to 54 N·m (40 lb ft).

2. Install the outer tie rod with the hex nut.

Tighten
Tighten the hex nut to 45 N·m (33 lb ft).

3. Inspect the vehicle. Refer to Preliminary Alignment Inspection and Straight Ahead Inspection .
4. Measure the wheel alignment.
5. If necessary, adjust the front toe. Refer to Front Toe Adjustment .