For 1990-2009 cars

## Front Fender Center Molding Replacement Hatchback

### Removal Procedure

1. Remove the fender. Refer to Front Fender Replacement
2. Remove the screws (1).
3. Disnengage the retaining tabs (2) and remove the fender molding (3) by pushing it out from the inside of the fender.

### Installation Procedure

1. Install the fender molding (3) by pushing the retaining tabs (2) in from the outside of the fender.
2. Install the screws (1).
3. Install the fender. Refer to Front Fender Replacement