For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Housing Assembly Retaining Bolts | 12 N·m | 106 lb in
Air Deflector Screws | 2 N·m | 18 lb in
A/C System Hose Connector Retaining Nut | 33 N·m | 24 lb ft
A/C Pressure Transducer | 8 N·m | 71 lb in
Blower Motor Screws | 6 N·m | 53 lb in
Blower Resistor Retaining Screws | 6 N·m | 53 lb in
Clutch Drive Shaft Bolt (SP10 Compressor) | 12-15 N·m | 106-133 lb in
Clutch Plate and Hub Assembly Nut (V5 Compressor) | 17 N·m | 13 lb ft
Compressor-to-Bracket Mounting Bolts | 27 N·m | 20 lb ft
Compressor Through Bolt | 10 N·m | 89 lb in
Condenser Pipe Connector Block-to-Receiver Dryer Nut | 10 N·m | 89 lb in
Expansion Valve Retaining Bolts | 12 N·m | 106 lb in
Heater/Air Distribution Case Assembly Retaining Screws | 8 N·m | 71 lb in
Liquid Pipe Connector Block-to-Condenser Retaining Bolt | 14 N·m | 10 lb ft
Liquid Evaporator Pipe Connector Block Retaining Nut | 15 N·m | 11 lb ft
Receiver Dryer Bolt | 14 N·m | 10 lb ft
Refrigerant Discharge Hose Support Clamp Bolt | 7 N·m | 62 lb in
Refrigerant Discharge Hose Connector Block Bolt | 16 N·m | 12 lb ft
Refrigerant Discharge Hose-to-Compressor Block Retaining Nut | 33 N·m | 24 lb ft
Refrigerant Suction Hose Connector Block Retaining Nut | 15 N·m | 11 lb ft
Upper Condenser Mount Nut | 3 N·m | 27 lb in