For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector.
3. Disconnect the electrical harness from the rear deck lid hinge arm.
4. Remove the bolts and the rear deck lid.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear deck lid with the bolts.

Tighten
Tighten the rear deck lid bolts to 10 N·m (89 lb in).

2. Connect the electrical harness to the rear deck lid hinge arm.
3. Connect the electrical connector.
4. Connect the negative battery cable.