For 1990-2009 cars

### Removal Procedure

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

1. Lift and suitably support the vehicle, allowing the front suspension to hang free.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the stabilizer shaft-to-knuckle nut and the shaft-to-link nut.
4. Disconnect the stabilizer shaft from the knuckle by removing the stabilizer shaft link assembly.

### Installation Procedure

1. Install the stabilizer shaft into the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer shaft-to-knuckle nut and the shaft-to-link nut.

Tighten
Tighten the stabilizer shaft link nuts to 50 N·m (37 lb ft).

3. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.