For 1990-2009 cars

1. Press the cluster shaft bearing onto the input shaft gear cluster.
2. Press the input driveshaft into the input shaft gear cluster assembly.
3. Install the snap ring at the base of the gear cluster.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the detent screw at the end of the input driveshaft.

Tighten
Tighten the input driveshaft detent screw to 15 N·m (11 lb ft).