For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel compartment.
2. Grip the glove box by both the upper and lower sides and pull it out of its housing.
3. Remove the filter cover by pressing in on the bottom retaining tab and pulling the cover down.
4. Remove the old passenger compartment air filter.

### Installation Procedure

Important: View the air flow arrows on the filter before installing to ensure you install the filter correctly.

1. Install the filter into housing.
2. Install filter cover.
3. Position glove box to instrument panel, making sure retaining tabs are engaged.
4. Close glove box.