For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using the diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC C1395: Fill and Bleed Not Complete

### Circuit/System Description

This procedure checks whether the brake system has been filled and bled properly.

### Conditions for Running the DTC

• | Vehicle speed is greater than 6 km/h (4 mph) with the brake pedal not applied.

| OR

• | Vehicle speed is greater than 15 km/h (9 mph) and the brake pedal is actuated.

### Conditions for Setting the DTC

• | Improper battery voltage

• | Brake system not properly bled

### Action Taken When the DTC Sets

• | The antilock brake system (ABS) is disabled.

• | The ABS warning indicator turns ON.

• | The electronic brake force distribution (EBD) is disabled.

### Conditions for Clearing the DTC

The condition for setting the DTC is no longer present and the DTC is cleared with a scan tool.

### Reference Information

#### Schematic Reference

Antilock Brake System Schematics

#### Connector End View Reference

Component Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

• | Connector Repairs

#### Scan Tool Reference

Electronic Brake Control Module Scan Tool Information

### Circuit/System Testing

1. Measure for 10-16 V across the battery terminals.

⇒ | If voltage is not as specified, check battery and charging system.

2. If voltage is as specified, bleed the brake system.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for EBCM and BPMV replacement, setup, and programming