For 1990-2009 cars

Table 1: | General Specifications
Table 2: | Performance - Manual Transmission
Table 3: | Manual Transmission
Table 4: | Transaxle Case Surface and Bearing Outer Races Clearance Table
Table 5: | Side Gear Axle Direction Play Table

#### General Specifications

Application | Specification
--- | ---
Metric | English
General

- Type - Forward Gear

Synchronized Mesh Type

- Type - Reverse Gear

Sliding Mesh Type

- Gear Ratio - 1st

3.417

- Gear Ratio - 2nd

1.950

- Gear Ratio - 3rd

1.280

- Gear Ratio - 4th

0.971

- Gear Ratio - 5th

0.758

- Gear Ratio - Reverse

3.273

- Final Drive Ratio

4.105

- Fluid Capacity

2.1 L

2.21 qt

- Fluid Classification

75W-85

GL-4

Service

- Clearance Between Gear and Synchronizer Ring - Limit

0.5 mm

0.020 in

- Clearance Between Gear and Synchronizer Ring - Standard

1.0 mm

0.039 in

- Clearance Between Sleeve and Shift Fork - Limit

1.0 mm

0.039 in

- Clearance Between Sleeve and Shift Fork - Standard

0.2-0.6 mm

0.008-0.024 in

- Key Groove Width of Synchronizer Ring - Limit - 1st Gear

10.0 mm

0.394 in

- Key Groove Width of Synchronizer Ring - Standard - 1st Gear

9.6 mm

0.378 in

- Key Groove Width of Synchronizer Ring - Limit - 2nd, 3rd, 4th Gear

10 mm

0.394 in

- Key Groove Width of Synchronizer Ring - Standard - 2nd, 3rd, 4th Gear

9.6 mm

0.378 in

- Key Groove Width of Synchronizer Ring - Limit - 5th Gear

9.8 mm

0.386 in

- Key Groove Width of Synchronizer Ring - Standard - 5th Gear

9.4 mm

0.370 in

- Shift Fork End Thickness for Low Speed Shift Fork - Limit - 1st-2nd Gear

8.1 mm

0.319 in

- Shift Fork End Thickness for Low Speed Shift Fork - Standard - 1st-2nd Gear

8.7 mm

0.343 in

- Shift Fork End Thickness for Low Speed Shift Fork - Limit - 3rd-4th Gear

7.2 mm

0.283 in

- Shift Fork End Thickness for High Speed Shift Fork - Standard - 3rd-4th Gear

7.8 mm

0.307 in

- Shift Fork End Thickness for Low Speed Shift Fork - Limit - 5th Gear

7.2 mm

0.283 in

- Shift Fork End Thickness for Shift Fork - Standard - 5th Gear

7.8 mm

0.307 in

- Speedometer Gear Ratio - Driven/Drive

17/18

0.944

- Thrust Free Play of Differential Side Gear

0.05-0.33 mm

0.002-0.013 in

#### Performance - Manual Transmission

Application | Specification
--- | ---
Metric | English
Gradeability | 0.4 (tan O)
Maximum Speed | 153 km/h | 95.1 mph
Minimum Turning Radius | 4.8 m | 15.7 ft

#### Manual Transmission

Application | Specification
--- | ---
Metric | English
Final Drive Ratio | 4.105:1
Gear Ratio

- 1st

3.417:1

- 2nd

1.950:1

- 3rd

1.280:1

- 4th

0.971:1

- 5th

0.758:1

- Reverse

3.273:1

Maker | DWMC
Oil Capacity | 2.1 L | 2.21 qt
Type or Model | Y4M

#### Transaxle Case Surface and Bearing Outer Races Clearance Table

Measured value | Shim thickness
--- | ---
0.33-0.37 mm (0.0130-0.0146 in) | 0.45 mm (0.0177 in)
0.38-0.42 mm (0.0147-0.0165 in) | 0.50 mm (0.0197 in)
0.43-0.47 mm (0.0169-0.0185 in) | 0.55 mm (0.0217 in)
0.48-0.52 mm (0.0189-0.0205 in) | 0.60 mm (0.0236 in)
0.53-0.57 mm (0.0209-0.0224 in) | 0.65 mm (0.0256 in)
0.58-0.62 mm (0.0228-0.0244 in) | 0.70 mm (0.0276 in)
0.63-0.67 mm (0.0248-0.0264 in) | 0.75 mm (0.0295 in)
0.68-0.72 mm (0.0268-0.0283 in) | 0.80 mm (0.0315 in)
0.73-0.77 mm (0.0287- 0.0303 in) | 0.85 mm (0.0335 in)
0.78-0.82 mm (0.0307-0.0323 in) | 0.90 mm (0.0354 in)
0.83-0.87 mm (0.0327-0.0343 in) | 0.90 mm (0.0354 in)
0.88-0.92 mm (0.0346-0.0362 in) | 1.00 mm (0.0394 in)
0.93-0.97 mm (0.0366-0.0382 in) | 1.05 mm (0.0413 in)
0.98-1.02 mm (0.0386-0.0402 in) | 1.10 mm (0.0433 in)
1.03-1.07 mm (0.0406-0.0421 in) | 1.15 mm (0.0453 in)

#### Side Gear Axle Direction Play Table

Application | Specification
--- | ---
Metric | English
Thrust Adjusting Shim | 0.90-0.95 mm | 0.0354-0.0374 in
1.00-1.05 mm | 0.0394-0.0413 in
1.10-1.15 mm | 0.0433-0.0453 in
1.20 mm | 0.0472 in
Thrust Free Play of Differential Side | 0.05-0.33 mm | 0.0020-0.0130 in