For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the timing belt. Refer to Timing Belt Replacement.

Note: Take extreme care to prevent any scratches, nicks, or damage to the camshaft. Such damage can impair vehicle operation.

3. Remove the camshaft gear. Refer to Camshaft Replacement.
4. Remove the timing belt automatic tensioner bolt.
5. Remove the timing belt automatic tensioner.
6. Remove the rear timing belt cover bolts.
7. Remove the rear timing belt cover.

### Installation Procedure

1. Install the rear timing belt cover.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear timing belt cover bolts and tighten to 10 N·m (89 lb in).
3. Install the timing belt automatic tensioner.
4. Install the timing belt automatic tensioner bolt and tighten to 20 N·m (15 lb ft).

Note: Take extreme care to prevent any scratches, nicks, or damage to the camshaft. Such damage can impair vehicle operation.

5. Install the camshaft gear. Refer to Camshaft Replacement.
6. Install the timing belt. Refer to Timing Belt Replacement.
7. Connect the negative battery cable.