For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Mounting Bracket Bolts | 37 N·m | 27 lb ft
Camshaft Position Sensor Bolts | 12 N·m | 106 lb in
Crankshaft Position Sensor Retaining Bolt | 6.5 N·m | 58 lb in
Electronic Ignition System Ignition Coil Retaining Bolts | 10 N·m | 89 lb in
Engine Control Module Bolts | 4 N·m | 35 lb in
Engine Coolant Temperature Sensor Retaining Bolt | 20 N·m | 15 lb ft
Evaporative Emission Canister Flange Bolt | 20 N·m | 15 lb ft
Evaporative Emission Canister Protective Cover | 8 N·m | 71 lb in
Evaporative Emission Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Fuel Filter Mounting Bracket Assembly Bolt | 4 N·m | 35 lb in
Fuel Pressure Regulator Retaining Screw | 12 N·m | 106 lb in
Fuel Rail Retaining Bolts | 25 N·m | 18 lb ft
Fuel Tank Retaining Bolts | 20 N·m | 15 lb ft
Idle Air Control Valve Retaining Bolts | 3 N·m | 27 lb in
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure Sensor Mounting Bracket Bolt | 4 N·m | 35 lb in
Manifold Absolute Pressure Sensor Retaining Bolts and Nuts | 8 N·m | 71 lb in
Oxygen Sensor Retaining Bolt | 42 N·m | 31 lb ft
Parking Brake Cable Retainer Clamps | 10 N·m | 89 lb in
Rear A/C Compressor Mounting Bracket Bolts | 35 N·m | 26 lb ft
Spark Plug Cover Bolts | 3 N·m | 27 lb in
Throttle Body Retaining Nuts | 15 N·m | 11 lb ft
Throttle Position Sensor Retaining Bolts | 2 N·m | 18 lb in