For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the luggage compartment lock.
3. Disconnect the electrical connector.
4. Disconnect the lock rod.
5. Disconnect the cable from the lock.

### Installation Procedure

1. Connect the cable to the lock.
2. Connect the lock rod.
3. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the luggage compartment lock with the screws.

Tighten
Tighten the luggage compartment lock screws to 6 N·m (53 lb in).

5. Connect the negative battery cable.