For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the intake manifold. Refer to Intake Manifold Replacement .
3. Disconnect the electrical connector at the KS.
4. Remove the KS.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the KS.

Tighten
Tighten the KS bolt to 20 N·m (15 lb ft).

2. Connect the electrical connector at the KS.
3. Install the intake manifold. Refer to Intake Manifold Replacement .
4. Connect the negative battery cable.