For 1990-2009 cars

#### Special Tools

EN-48356 Engine Fixture

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Install EN-48356 fixture .
3. Remove the engine mount bolts (2) and nuts (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine mount bolts (2) and nuts (1) and tighten to 55 N·m (40.5 lb ft).
2. Remove EN-48356.
3. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.