For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment lid.
2. Remove the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement .
3. Remove the weatherstrip from around the gutter.

### Installation Procedure

1. Install the weatherstrip onto the gutter flange.
2. Inspect the weatherstrip. Make sure that the clinch is completely seated onto the flange.
3. Using a water hose without a nozzle, test the rear deck lid to make sure that no leaks are present.
4. Install the luggage compartment rear trim panels. Refer to Rear Compartment Trim Panel Replacement .