For 1990-2009 cars

### Removal Procedure

Note: To remove the power steering pump belt, do remove the accessory belt in advance.

1. Rotate the tensioner star-nut (1 and remove the accessory belt.
2. Remove the power steering belt. Refer to Power Steering Pump Replacement.
3. Remove the accessory belt tensioner (1.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the accessory belt tensioner (1) and tighten to 50 N·m (36.8 lb ft).
2. Install the power steering belt. Refer to Power Steering Pump Replacement.
3. Rotate the tensioner star-nut (1) and install the accessory belt.
4. Install the engine front shield at the position of right front wheel.