For 1990-2009 cars

#### Tools Required

GE-42910 Yoke Adjusting Tool

### Adjustment Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Ensure the steering wheel and the front wheels are in the straight ahead position.
3. Remove the steering gear. Refer to Steering Gear Replacement.
4. Loosen the locknut (1).

Notice: Refer to Fastener Notice in the Preface section.

5. Use the GE-42910 in order to tighten the yoke plug (2).

Tighten
Tighten the yoke plug to 5 N·m (44 lb in).

6. Loosen the yoke plug by 45 degrees.
7. Hold the yoke plug stationary and tighten the locknut (1).

Tighten
Tighten the locknut to 44 N·m (32 lb ft).

8. Install the steering gear. Refer to Steering Gear Replacement.
9. Drive the vehicle and ensure the steering system returns to the straight ahead position.