For 1990-2009 cars

#### Special Tools

• | EN-49074 Universal Valve Spring Compressor

• | EN-49155 Valve Spring Compressing Adapter

• | EN-49154 Adapter-Cylinder Pressure

• | KM-845 Suction Device

### Removal Procedure

1. Remove the camshaft. Refer to Camshaft Replacement.
2. Remove the valve tappet using KM-845 suction device .
3. Remove the spark plugs and then install the EN-49154 pressure .
4. Apply the compressed air to the adapter to avoid dropping of valves in the cylinders inside.
5. Install EN-49074 compressor and EN-49155 adapter .
6. Remove the valve key (1).
7. Remove the valve springs (3), retainers (2), and seals (4).
8. Remove the EN-49074 compressor and EN-49155 adapter .

### Installation Procedure

1. Install the seals (4), retainers (2), and valve spring (3).
2. Install EN-49074 compressor and EN-49155 adapter .
3. Install the valve key (1).
4. Install the valve tappet using KM-845 .
5. Install the camshaft. Refer to Camshaft Replacement.