For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the floor console. Refer to Front Floor Console Replacement.
3. Remove the shift select lever knob.
4. Disconnect the connectors.
5. Remove the shift select cover from the shift select housing.

### Installation Procedure

1. Connect the connectors to the shift select cover.
2. Install the shift select cover to the hole.
3. Install the shift select lever knob.
4. Install the floor console. Refer to Front Floor Console Replacement.
5. Connect the negative battery cable.