For 1990-2009 cars

### Circuit Description

When the ignition switch is turned to ON, the sensing and diagnostic module (SDM) will perform a turn-on test to diagnose critical malfunctions within the SDM itself.

Upon passing this test, ignition and deployment loop voltages are measured to ensure that they are within their normal voltage ranges. The SDM monitors the voltages at the driver low and the passenger low to detect shorts to ground or voltage in the deployment loops.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC 011 Driver Pretensioner Deployment Loop Short To Ground

### Conditions for Running the DTC

Ignition voltage is within the normal operating voltage range.

### Conditions for Setting the DTC

• | The belt pretensioner wiring of the driver high is shorted to ground.

• | The belt pretensioner wiring of the driver low is shorted to ground.

### Action Taken When the DTC Sets

The SDM commands the AIR BAG indicator ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section. Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section. Schematic Reference: SIR Schematics Connector End View Reference: SIR Connector End Views
1 | Did you perform a Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Disconnect the negative battery cable.
2. Wait 1 minute for the sensing and diagnostic module (SDM) capacitor to discharge.
3. Visually inspect the SIR wiring harness.

Is there any visible damage to the SIR wiring harness?

--

Go to Step 3

Go to Step 4

3 | Replace the SIR wiring harness. Did you complete the repair? | -- | Go to Step 7 | --
4 |

1. Disconnect the electrical connector from the driver seat belt pretensioner module.
2. Disconnect the electrical connector at the SDM.
3. Measure the resistance between ground and each of the terminals at the SDM side of the wiring harness connector for the driver seat belt pretensioner module.

Does the resistance measure less than the specified value?

∞

Go to Step 3

Go to Step 5

5 |

1. Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement .
2. Connect the negative battery cable.
3. Use the scan tool in order to clear the DTCs.
4. Perform the Diagnostic System Check - Vehicle .

Is DTC 011 still shown as a current fault?

--

Go to Step 6

Go to Step 7

6 | Replace the driver seat belt pretensioner module. Refer to Front Seat Belt Replacement . Did you complete the repair? | -- | Go to Step 7 | --
7 |

1. Reconnect all SIR components.
2. Verify that all components, connectors and connector position assurances (CPAs) are properly mounted.
3. Use the scan tool in order to clear the DTCs.
4. Operate the vehicle within the Conditions for Running the DTC, as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK