For 1990-2009 cars

## Center Pillar Upper Trim Panel Replacement Hatchback

### Removal Procedure

1. Remove the bolt and the upper front seat belt anchor.
2. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Remove the screws and the seat belt bracket.
4. Pry off the upper center pillar trim panel.

### Installation Procedure

1. Install the upper center pillar trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the seat belt bracket with the screws.

Tighten
Tighten the seat belt bracket screws to 10 N·m (89 lb in).

3. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Install the upper front seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).

## Center Pillar Upper Trim Panel Replacement Notchback

### Removal Procedure

1. Remove the bolt and the upper front seat belt anchor.
2. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Pry off the upper center pillar trim panel.

### Installation Procedure

1. Install the upper center pillar trim panel.
2. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper front seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).