For 1990-2009 cars

### Removal Procedure

1. Locate the four locking tabs on the generator cover.
2. Using a screwdriver (3), carefully pry the generator cover locking tabs (2) in four places and remove the generator cover (1).

Important: Screw (1) is slightly shorter then the other four screws (2).

3. Remove the 5 screws (1 and 2) that retain the voltage regulator (3) and the rectifier (4) to the generator.
4. Carefully lift up the rectifier (2) and remove the voltage regulator (1).

### Installation Procedure

1. Depress the voltage regulator (2) brushes and insert tube (1) into the opening to keep brushes in the depressed position.
2. Install the voltage regulator (1) on the generator and ensure the battery ring terminal (2) is positioned on the battery stud.
3. Remove the brush tube (3).

Important: Screw (1) is slightly shorter then the remaining 4 screws (2) and must be installed in the position shown.

4. Install the 5 screws (1 and 2) on the generator.

Tighten
Tighten the rectifier and voltage regulator retaining screws to 3 N·m (26 lb in).

5. Snap the generator cover (1) into place.