For 1990-2009 cars

#### Tools Required

• | DT 46464 (DW240-160) Transaxle Case Outer Tapered Roller Bearing Race Adapter

• | DT 46465 (DW240-170) Adapter Handle

Important: Press-fit the outer tapered roller bearing race until it contacts the transaxle housing.

1. Install a new outer tapered roller bearing race into the transaxle housing.

Important: Press-fit the shim until it contacts the transaxle case.

Important: Install a shim of the same thickness as the one removed.

2. Install the shim to the transaxle case.
3. Using DT 46464 (2) and DT 46465 (1), press in a new outer tapered roller bearing race into the transaxle case.
4. Using a press, install the counter driven gear.
5. Using a press, install a new tapered roller bearing on the transaxle case side.
6. Using a press, install a new tapered roller bearing on the transaxle housing side.