For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
3. Remove the screws and the front speaker.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front speaker with the screws and tighten to 3.5 N·m (31 lb in).
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
4. Connect the negative battery cable.