For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the ignition cables.
3. Disconnect the ignition cable harness connector.
4. Remove the ignition coil retaining bolts (2).
5. Remove the ignition coil (1).
6. Remove the ignition coil bracket retaining bolts (2).
7. Remove the ignition coil bracket (1).

### Installation Procedure

1. Install the ignition coil bracket (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the ignition coil bracket retaining bolts (2) and tighten to 10 N·m (7.3 lb ft).
3. Install the ignition coil (1).
4. Install the ignition coil retaining bolts (2) and tighten to 10 N·m (7.3 lb ft).
5. Connect the ignition coil harness connector.
6. Connect the ignition cables.
7. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.