For 1990-2009 cars

Table 1: | Battery Voltage Specifications

Application | Description
--- | ---
L4 Engine
Cold Cranking Amps | 550 amps
Load Test | 270 amps
RC - Minimum | 90 minutes
Replacement | 85B-60

#### Battery Voltage Specifications

Application | Specification
--- | ---
Metric | English
Minimum Voltage:

- 9.6 V

21°C

70°F

- 9.4 V

20°C

68°F

- 9.1 V

0°C

32°F

- 8.8 V

-10°C

14°F

- 8.5 V

-18°C

0°F

- 8.0 V

Below -18°C

Below 0°F