For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the PCV hose.
3. Remove the cylinder head cover bracket and bolts.
4. Remove the spark plug cable cover (1).
5. Disconnect the spark plug cable.
6. Remove the cylinder head cover retaining bolts.
7. Remove the cylinder head cover (1) with the gasket.

### Installation Procedure

1. Install the cylinder head cover (1) with the gasket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the cylinder head cover retaining bolts.

Tighten
Tighten the cylinder head cover bolts to 10 N·m (7.4 lb ft).

3. Connect the ignition cable.
4. Install the ignition cable cover (1).
5. Install the cylinder head cover bracket retaining bolts.

Tighten

• | Tighten the cylinder head cover bracket bolts to 10 N·m (7.4 lb ft).

• | Tighten the spark plugs cable cover bolts to 10 N·m (7.4 lb ft).

6. Connect the PCV hose.
7. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.